**WEIGHT AND BALANCE REVISION RECORD**

DATE: 24 MAY 2014

SUPERCEEDS FORM DATED: 20 OCT 2008

AIRCRAFT: N162PT

SERIAL #: 15285278

MAKE: Cessna

MODEL: 152

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ITEM | IN | OUT | WEIGHT | ARM | MOMENT |
| Skytec 122-LN/EC Starter | XX |  | 9.6 | -28.6 | -274.56 |
| Original Cessna starter |  | XX | -15.1 | -28.6 | 431.86 |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| Change Total |  |  | -5.5 |  | 157.30 |
| Previous A/C BEW dated 20 OCT 2008 |  |  | 1138.6 | 29.80 | 33928.43 |
| New A/C BEW, ARM & MOMENT |  |  | 1133.1 | 30.08 | 34085.73 |

See aircraft flight manual for center of gravity limitations.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Authorized Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Certificate type and #

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date